DBH05-DBH20-DBH09R

VOX = voice operated transmitter it allows you to transmit with you voice without pressing the button.

CA = call allows you to adjust different tones for calling the operator from the same channel.

REP = A repeater is a tool to communicate over a large distances.

RO = roger beep means a tone added to the end of broadcast, it indicates that the user/operator has conclude speaking.

BELL =symbol on the display = turn off/on the beep when using any buttons.

DCM = dual channel monitoring you can monitor between two channels eg: 1 to 22 or 50 to55.

DCS = DCS is a digital extension of CTCSS. It provides 104 extra, digitally coded, squelch codes that follow after the 38

CTCSS codes. CTCSS 1-38, followed by DCS 1-104.

TO = time out is when the unit turns off after 30min or 60min when activated.