MUTE WIRE FOR THE IN CAR CB

MUTE WIRE

The way the mute wire works is if you look at the back of your car stereo, there may be a muting input wire that allows you connect the blue wire from the 477a radio to the mute wire on the radio. (The mute wire colour on the radio may vary depending on the type and model of your radio.)

The black wire from the RX mute pair (BLACK/BLUE) black is grounded to the chassis of your car radio.