HOW TO INSTALL THE FIRWARE FIX

ON THE HDDVR202

Make sure the unit is fully charged before proceeding

Load the Bin file on to the micro sd card

Insert the card in on the HDDVR202

Power the unit on

The screen will boot up when the firmware is completed

Please make sure the sd card is formatted once completed